

MaxAir supports zones based on their type, these types define the basic capability of the zone:


* Associated with a sensor, zone controller relays and system controller relays
* Associated with a sensor and zone controller relays
* Associated with only zone controller relays
* Associated with a sensor and system controller relays

A number of Zone Types are pre-defined:

* Heating – has a temperature sensor, zone controller relays and a system controller relay
* Water – has a temperature sensor, zone controller relays and a system controller relay
* Immersion – has a temperature sensor and zone controller relays
* Switch – has system controller relays
* HVAC – has a temperature sensor and system controller relays
* Humidity - has a humidity sensor and zone controller relays
* Binary – has a ON/OFF sensor and zone controller relays
* HVAC-M – has a temperature sensor, zone controller relays and system controller relays

The currently defined Zone Types can be viewed from the ‘Zone Type’ menu option in the ‘Settings/Node and Zone Configuration’ menu.

Zone Types can be deleted by clicking on the ‘trash’ icon or addition ones added by clicking on the ‘Add Type’ button.

Enter a name for the new Zone the and select the appropriate ‘Category’ from the dropdown list, finally click on the ‘Save’ button.